**HOW TO SPECIFY**

**Model UNI-PD**

**STAMPED SQUARE PERFORATED DOWNBLAST CEILING DIFFUSERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model UNI-PD Square Perforated Downblast Ceiling Diffusers** of the sizes and capacities as shown on the plans and air distribution schedules. The diffuser shall be manufactured from corrosion-resistant steel and include a stamped one-piece construction outer cone with an inner core that has a square face plate that includes perforated holes in a spherical pattern. The perforations shall be 3/8" (10) diameter holes on 5/8" (16) centers. The finish shall be AW Appliance White (optional finishes are available).The manufacturer shall provide published performance data for the diffuser, which shall be tested in accordance with ANSI/ASHRAEStandard 70-2006. |

**Model UNI-AD**

**STAMPED SQUARE RADIAL VANE DOWNBLAST CEILING DIFFUSERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model UNI-AD Square Adjustable Downblast Ceiling Diffusers** of the sizes and capacities as shown on the plans and air distribution schedules. The diffuser shall be manufactured from corrosion-resistant steel and include a stamped one-piece construction outer cone with an inner core that has a square face plate and includes a round, easily adjustable radial vane in the center. The radial vane shall have a ring operator that allows for pole operation. The finish shall be AW Appliance White (optional finishes are available).The manufacturer shall provide published performance data for the diffuser, which shall be tested in accordance with ANSI/ASHRAEStandard 70-2006. |