**HOW TO SPECIFY**

**Models 7145V(-O), 7145H(-O), 71FV(-O), 71FH(-O)**

**AIRFOIL BLADE RETURN GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **7145H, 7145V, 71FH** or **71FV Airfoil Blade Airfoil Blade Return Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grilles shall have extruded aluminum fixed blades that are airfoil shaped and spaced on 3/4" (19) centers. The frame is to be constructed from heavy gauge extruded aluminum with reinforced mitered corners. The finish shall be AW Appliance White (optional finishes are available).(Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel (aluminum is optional) and operable from the face of the grille, shall be provided with all units.The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |