**HOW TO SPECIFY**

**Models 51D30H-HD(-O), 51D30V-HD(-O), 51D15H-HD(-O), 51D15V-HD(-O), 51DFH-HD(-O), 51DFV-HD(-O)**

**ALUMINUM HEAVY DUTY BAR SUPPLY GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**  Furnish and install **Nailor Model** (select one) **51D30H-HD, 51D30V-HD, 51D15H-HD, 51D15V-HD, 51DFH-HD** or **51DFV-HD Aluminum Heavy Duty Bar Supply Grilles** with rear deflection vanes of the type and size as shown on the plans and air distribution schedules. The grille shall have extruded aluminum reinforced blades and welded frame. The front bars are to be fixed on 1/2" (13) centers and the rear deflection vanes are to be adjustable on 3/4" (19) centers. The finish shall be AW Appliance White (optional finishes are available).  (Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel (aluminum is optional) and operable from the face of the grille, shall be provided with all units.  The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |